Issue July 15, 2013
Architects’ Specifications for
myMix, networkable, decentralized digital mixing and multi-track recording system
Products:
myMix – 2 channel input, stereo output, 16 channel mixer and multi-track recorder
myMix INSTALL – 2ch input, stereo output, 16 ch mixer for permanent installation
WMB01 – In-wall mounting box for myMix INSTALL
IEX-16L – 16 channel line level input expander for myMix systems
IEX-16L-A - 16 channel input expander for myMix systems analogue and digital inputs
myMix CONTROL - web browser operated remote control software for myMix systems
POWER8 – preconfigured Cisco 8 port POE Switch for myMix with 2 GB Ports
POWER12 – preconfigured Cisco 24 port POE Switch with POE budget for 12 myMix, 4 GB ports
Note for Ethernet network:
myMix utilizes off-the-shelf Fast Ethernet networking hardware. myMix network protocol is a proprietary,  Ethernet AVB-like protocol, customized to work with conventional, preconfigured Fast Ethernet switches. 
To guarantee the performance of the myMix system, it is recommended  to operate the myMix devices on an exclusive or isolated network, or at least an individual subnet and not mix it with other data traffic.
Depending on the existing network infrastructure myMix can be integrated in to existing networks.
Basic Specs/Requirements:
Discovery: VLAN1
IP addressing:  IPv4 Link-Local
Audio transport: VLAN 2  (conforms with IEEE1722 with some exception, e.g. IGMP multicast filtering)
Time Sync: IEEE1588-2008, using layer 2 transport, Media Clock PTP grand master.
Channel selection (for systems with more than 16 audio channels>):  IGMP snooping (v2). 
To prevent the myMix devices from data overflow unregistered multicast needs to be filtered, the Media Clock (PTP) needs to be exempt from filtering. 

Architects‘ Specifications myMix networkable mixer and recorder

Networkable, decentralized digital audio mixing and multi track recording device
Networkable, decentralized 16/2 digital mixing console for self-contained operation as well as use in 100MB Fast Ethernet networks. Audio transport in uncompressed 24-bit, 48kHz quality, in accordance to IEEE1722, with proprietary network overhead. Intuitive and clear operation with push-button encoder. All functions and network channel names displayed on a full color LCD Display with 480x272 pixels. Two audio inputs for microphone and line level signals, configurable as two dual mono, or one stereo signal, adjustable gain, two-color level indicator LED for signal present and peak, switchable phantom power for both channels. Stereo mix signal available as balanced line level output on ¼-inch TRS in addition to headphone mini-jack. Switchable 4-band fully parametric equalizer for stereo output signal. Local audio inputs as well as the stereo mix can be sent to the network, while an individual selection of 8 signal pairs (max. 16 mono channels) can be received from the network. Selected audio signals can be soloed and muted as well as adjusted in volume, tone control, effect send and panorama. Integrated stereo effect processor with 6 presets for rooms/reverb and one adjustable delay. All myMix settings, including channel selection, input mode and naming are automatically stored in the current profile. Up to 20 different profiles can be created, named and recalled at any time. Integrated card reader for optional SD/SDHC cards, allows firmware updates and multi-track recording of the selected audio channels and the stereo mix by the push of a single button. Audio files recorded as time stamped WAV file (24-Bit, 48kHz). Playback of the multi-track audio files with complete adjustment of all parameters from the myMix mixer. Play Along mode to mix the signal of the two local inputs with up to 14 tracks from the memory card. All signals on the network can be labeled and are displayed to all network users with their names. New network participants (or audio signals) are automatically detected and displayed with their names to all users. Remote configuration and editing or parameters with optional myMix CONTROL software. Power is supplied via external 24V psu or Power-Over-Ethernet (15.4 watts) from the switch. Number of possible audio channels in the network more than 250 using a suitable Fast Ethernet switch. Included detachable microphone stand adaptor for attachment to conventional microphone stands. Optional available with Studio Modification for highly noise sensitive environments.
Technical Data:
Input Impedance (Microphone/Line-Level):		2 kOhms / 20 kOhms
Input Gain Microphone/ Line:				variable +4 to +60 dB / -16 to + 40dB
Max. Input Level (Microphone/Line):			+14 dBu / +34 dBu
Output Impedance and max. Level:			75 Ohm, + 21 dBu
Headphone Amplifier:					280mW into 50 Ohms, 16 Ohms min.
Frequency Response and THD+N (1 kHz):		20 Hz - 20 kHz (+0, -1 dB), <0,022%
Signal-to-Noise Ratio:					>104 dB
Crosstalk:						< -80 dB
Mute:							> 100dB
Network Audio Data:					24-Bit, 48kHz
Network Type:						Fast Ethernet (100BASE-TX)
Data format recording:					wav-File, 24-Bit, 48kHz
Networking Protocol:					Proprietary (prelim. Ethernet AVB)
Memory Card Format:					SD/SDHC Format (SDA 2.0 compatible)
Network Connector:					1 RJ45 (Amphenol)
Audio Inputs:						2 XLR-TRS Combo (Neutrik), balanced
Audio Outputs:						2 Stereo TRS (Neutrik), balanced
Headphone Output:					1/8” Mini-TRS (3,5mm), Switchcraft
Dimensions (W x H x D):				134 mm x 171 mm x 60 mm
							(5.3” x 6.7” x 2.4”)
Weight, net:						0,5 kg (1.1lbs)
External PSU (included):				output 24V, 0,5A, input 100-240V, 50/60Hz
Microphone Stand Adapter:				Included

Proposed Device:
Make:							MOVEK
Model:							myMix
Price:							__________
Price, Installation:					__________
Price for Studio Modification (-10dB):			__________ 

Architects‘ Specifications 
myMix Install- networkable mixer and recorder for permanent installation

Networkable, decentralized digital audio mixing and multi track recording device for permanent installation
Networkable, decentralized 16/2 digital mixing console for self-contained operation as well as use in 100MB Fast Ethernet networks. Audio transport in uncompressed 24-bit, 48kHz quality, in accordance to IEEE1722, with proprietary network overhead. Intuitive and clear operation with push-button encoder. All functions and network channel names displayed on a full color LCD Display with 480x272 pixels. Two audio inputs for microphone and line level signals, configurable as two dual mono, or one stereo signal, adjustable gain, two-color level indicator LED for signal present and peak, switchable phantom power for both channels. Stereo mix signal available as balanced line level output on ¼-inch TRS in addition to headphone mini-jack. Switchable 4-band fully parametric equalizer for stereo output signal. Local audio inputs as well as the stereo mix can be sent to the network, while an individual selection of 8 signal pairs (max. 16 mono channels) can be received from the network. Selected audio signals can be soloed and muted as well as adjusted in volume, tone control, effect send and panorama. Integrated stereo effect processor with 6 presets for rooms/reverb and one adjustable delay. All myMix settings, including channel selection, input mode and naming are automatically stored in the current profile. Up to 20 different profiles can be created, named and recalled at any time. Integrated card reader for optional SD/SDHC cards, allows firmware updates and multi-track recording of the selected audio channels and the stereo mix by the push of a single button. Audio files recorded as time stamped WAV file (24-Bit, 48kHz). Playback of the multi-track audio files with complete adjustment of all parameters from the myMix mixer. Play Along mode to mix the signal of the two local inputs with up to 14 tracks from the memory card. All signals on the network can be labeled and are displayed to all network users with their names. New network participants (or audio signals) are automatically detected and displayed with their names to all users. Remote configuration and editing or parameters with optional myMix CONTROL software. Power is supplied via external 24V  or Power-Over-Ethernet (15.4 watts) from the switch. Number of possible audio channels in the network more than 250 using a suitable Fast Ethernet switch. Metal housing with flat glass panel and  Euro block screw terminal on the rear panel, suitable for desk- or wall mounting.
Technical Data:
Input Impedance (Microphone/Line-Level):		2 kOhms / 20 kOhms
Input Gain Microphone/ Line:				variable +4 to +60 dB / -16 to + 40dB
Max. Input Level (Microphone/Line):			+14 dBu / +34 dBu
Output Impedance and max. Level:			75 Ohm, + 21 dBu
Headphone Amplifier:					280mW into 50 Ohms, 16 Ohms min.
Frequency Response and THD+N (1 kHz):		20 Hz - 20 kHz (+0, -1 dB), <0,022%
Signal-to-Noise Ratio:					>104 dB
Crosstalk:						< -80 dB
Mute:							> 100dB
Network Audio Data:					24-Bit, 48kHz
Network Type:						Fast Ethernet (100BASE-TX)
Data format recording:					wav-File, 24-Bit, 48kHz
Networking Protocol:					Proprietary (prelim. Ethernet AVB)
Memory Card Format:					SD/SDHC Format (SDA 2.0 compatible)
Network Connector:					1 RJ45 (Amphenol)
Audio Inputs:						Euro block, screw terminal (balanced)
Audio Outputs:						Euro block, screw terminal (balanced)
Headphone Output:					1/8” Mini-TRS (3,5mm)
Dimensions (W x H x D):				216 mm x 167 mm x 55 mm
							(8.5” x 6.6” x 2.2”)
Weight, net:						1,1 kg (2.4 lbs)
External power 	(or POE)				24V, 0,5A DC

Proposed Device:
Make:							MOVEK
Model:							myMix INSTALL
Price:							__________
Price, Installation:					__________

WMB01 – Wall-mount box for myMix INSTALL
Solid metal box for in-wall mounting of myMix INSTALL. For use in dry- and brick walls.

Dimensions (W x H x D):				194 mm x 152 mm x 70 mm
							(7.6” x 6.0” x 2.8”)
Weight, net:						0,5 kg (1.1lbs)

Proposed Device:
Make:							MOVEK
Model:							WMB01
Price:							__________
Price, Installation:					__________

Architects’ Specifications IEX-16L Input Expander

16 Channel Input Expander for networkable, decentralized digital audio mixing system
16 Channel input expander for myMix decentralized audio mixing system. 16 inputs for analog audio line level signals on two DB25 connectors. 24-Bit AD-conversion and transmission to Fast Ethernet network for use with myMix digital mixing and recording devices. Configuration of input channels via external myMix device or optional myMix CONTROL software. Input channels can be configured in pairs as a dual-mono or single stereo signal. Switchable digital gain of +6dB and +12dB per channel. Channel naming with up to 16 alphanumeric characters for automatic display on the myMix network. 100BASE-TX network interface for transmission of audio data and configuration, additional configuration port for system configuration and locking/unlocking of the configuration screen. Automatically stored configuration settings. Automatically managed system master clock. 16 two-color LEDs for signal present and peak. 19“ metal housing for rack mounting (1U), external power supply. 
Technical Data:
Input Impedance (Line-Level):				20 kOhm
Input Gain:	 					switchable: 0, +6, +12 dB
Max. Input Level:					+20 dBu
Frequency Response & THD+N (1 kHz):			20 Hz - 20 kHz (+0, -1 dB), <0,022%
Signal-to-Noise Ratio:					>104 dB
Network Audio Data:					24-Bit, 48kHz
Network Type:						Fast Ethernet (100BASE-TX)
Network Protocol:					Proprietary (prelim. version of Ethernet AVB)
Network Connector:					1 RJ45 (Amphenol)
Configuration Port:					1 RJ 45 
Audio Inputs:						2 x 8 Line Level balanced, DB25 multipin
Dimensions (W x H x D):				483 mm x 45 mm x 145 mm
							(19“ x 1.75“ x 5“)
Weight, net:						2,7 kg (6 lbs)
External PSU (included):				output 24V, 0,5A, input 100-240V, 50/60Hz

Proposed Device:
Make:							MOVEK
Model:							IEX-16L
Price:							__________
Price, Installation:					__________

Architects’ Specifications IEX-16L-A Input Expander

16 Channel Input Expander for networkable, decentralized digital audio mixing system
16 Channel input expander for myMix decentralized audio mixing system. 16 inputs for digital signals in ADAT format switchable for analog audio line level signals on two DB25 connectors. 24-Bit AD-conversion and transmission to Fast Ethernet network for use with myMix digital mixing and recording devices. Configuration of input channels via external myMix device or optional myMix CONTROL software. Input channels can be configured in pairs as a dual-mono or single stereo signal. Switchable digital gain of +6dB and +12dB per channel. Channel naming with up to 16 alphanumeric characters for automatic display on the myMix network. 100BASE-TX network interface for transmission of audio data and configuration, additional configuration port for system configuration and locking/unlocking of the configuration screen. Automatically stored configuration settings. Automatically managed system master clock. 16 two-color LEDs for signal present and peak. 19“ metal housing for rack mounting (1U), external power supply. 
Technical Data:
Audio Inputs:						2 x 8 Line Level balanced, DB25 
Input Impedance (Line-Level):				20 kOhm
Digital Inputs						2 x 8ch, ADAT€® - optical-TOSLINK
Input Gain:	 					switchable: 0, +6, +12 dB
Max. Input Level:					+20 dBu
Frequency Response & THD+N (1 kHz):			20 Hz - 20 kHz (+0, -1 dB), <0,022%
Signal-to-Noise Ratio:					>104 dB
Network Audio Data:					24-Bit, 48kHz
Network Type:						Fast Ethernet (100BASE-TX)
Network Protocol:					Proprietary (prelim. version of Ethernet AVB)
Network and Config Port Connector:			 RJ45 (Amphenol)
Dimensions (W x H x D):				483 mm x 45 mm x 145 mm
							(19“ x 1.75“ x 5“)
Weight, net:						2,7 kg (6 lbs)
External PSU (included):				output 24V, 0,5A, input 100-240V, 50/60Hz

Proposed Device:
Make:							MOVEK
Model:							IEX-16L-A
Price:							__________
Price, Installation:					__________

Architects’ Specifications myMix CONTROL
Web browser operated Remote Control Software for myMix Systems
Web browser operated remote control software for myMix systems using the myMix PLUG as network interface and web server. Allows remote configuration and editing of myMix and IEX16 devices including: input/output configuration and channel naming, channel selection, effects, master eq settings and mix functions (i.e. level, effect send, tone control and panorama/balance, solo and mute. Allows individual locking of myMix parameters including: solo, mute, master volume, zero mix, settings, profiles, delete profile, create profile, rename profile, master eq, effects, sessions, delete session, rename session, remote channel select, remote devices, preferences, administration, recording, master mute and total lock. Complete project files including all devices with all settings as well as individual unit settings, profiles and preferences can  be saved  to and uploaded from internal memory, attached USB drive, or the hard disk of the client computer. Profiles can be changed individually or globally for all myMix devices on the network. Access password protected for two level of users (administrator and general user).
The web browser operated software is hosted on a 1.2GHz computer with Linux OS, 512MB RAM, one GB- Ethernet port, two USB2.0 interfaces and a Wi-Fi  802.11b/g access point. 
myMix PLUG (containing myMix CONTROL web browser interface)
Dimensions (W x D x H) 				65 x 96 x 48.5 mm (2.6" x 3.8" x 1.9")
Power Requirements					AC 100-240V, 50/60Hz
Power Consumption					max. 20W

Proposed Device:
Make:							MOVEK
Model:							myMix CONTROL
Price:							__________
Price, Installation:					__________

Architects‘ Specifications for POWER8 ( preconfigured Cisco SF302-08MP)
Fast Ethernet Switch for myMix System with POE for 8 myMix units and uplink port
Web Managed Fast Ethernet Switch compatible to 802.1x. Eight 100BASE-TX ports each with 15.4W POE (Power-Over-Ethernet). Two 100/1000BASE TX Ports. Configured for use with myMix. G2 configured as uplink port. External power supply, fan-less operation, 19“ rack mount kit included. .
Technical Data:
Fast Ethernet (100MB/s) Ports:					8
Gigabit Ports (100/1000MB/s):					2
Mini GBIC ports:						2
POE Budget							124W
Switch Capacity:						5.6 GBps
IGMP Snooping							V2, V3
Multicast Groups:						256
Compliant to:
IEEE 802.3 10BASE-T Ethernet, IEEE 802.3u 100BASE-TX Fast Ethernet, IEEE 802.3ab 1000BASE-T 
Gigabit Ethernet, IEEE 802.3ad LACP, IEEE 802.3z Gigabit Ethernet, IEEE 802.3x, IEEE 
802.1D (STP, GARP, und GVRP),IEEE 802.1Q/p VLAN, IEEE 802.1w RSTP, IEEE 802.1s Multiple STP, 
IEEE 802.1X Port Access Authentication, IEEE 802.3af, IEEE 802.3at, RFC 768, RFC 783, RFC 791, 
RFC 792, RFC 793, RFC 813, RFC 879, RFC 896, RFC 826, RFC 854, RFC 855, RFC 856, RFC 858, 
RFC 894, RFC 919, RFC 922, RFC 920, RFC 950, RFC 951, RFC 1042, RFC 1071, RFC 1123, RFC 
1141, RFC 1155, RFC 1157, RFC 1350, RFC 1533, RFC 1541, RFC 1542, RFC 1624, RFC 1700, RFC 
1867, RFC 2030, RFC 2616, RFC 2131, RFC 2132, RFC 3164, RFC 3411, RFC 3412, RFC 3413, RFC 
3414, RFC 3415, RFC 2576, RFC 4330, RFC 1213, RFC 1215, RFC 1286, RFC 1442, RFC 1451, RFC 
1493, RFC 1573, RFC 1643, RFC 1757, RFC 1907, RFC 2011, RFC 2012, RFC 2013, RFC 2233, RFC 
2618, RFC 2665, RFC 2666, RFC 2674, RFC 2737, RFC 2819, RFC 2863, RFC 1157, RFC 1493, RFC 
1215, RFC 3416

Proposed Device:
Make:							CISCO
Model:							SF302-08MP
Price:							__________
Price configuration for myMix:				__________
Price Installation:					__________

Architects‘ Specifications for POWER12 ( preconfigured Cisco SF300-24P)
Fast Ethernet Switch for myMix System with POE for 12 myMix units and uplink port
Web Managed Fast Ethernet Switch compatible to 802.1x. 24 100BASE-TX ports, 12 with each 15.4W POE (Power-Over-Ethernet). Four 100/1000BASE TX Ports. Configured for use with myMix including four GB uplink ports. Internal power supply with fan, 19“, 1U rack mount.
Technical Data:
Fast Ethernet (100MB/s) Ports:					24
Gigabit Ports (100/1000MB/s):					4
Mini GBIC ports:						2
POE Budget							180W
Switch Capacity:						12.8 GBps
IGMP Snooping							V2, V3
Multicast Groups:						256
Compliant to:
IEEE 802.3 10BASE-T Ethernet, IEEE 802.3u 100BASE-TX Fast Ethernet, IEEE 802.3ab 1000BASE-T 
Gigabit Ethernet, IEEE 802.3ad LACP, IEEE 802.3z Gigabit Ethernet, IEEE 802.3x Flow Control, IEEE 
802.1D (STP, GARP, und GVRP),IEEE 802.1Q/p VLAN, IEEE 802.1w RSTP, IEEE 802.1s Multiple STP, 
IEEE 802.1X Port Access Authentication, IEEE 802.3af, IEEE 802.3at, RFC 768, RFC 783, RFC 791, 
RFC 792, RFC 793, RFC 813, RFC 879, RFC 896, RFC 826, RFC 854, RFC 855, RFC 856, RFC 858, 
RFC 894, RFC 919, RFC 922, RFC 920, RFC 950, RFC 951, RFC 1042, RFC 1071, RFC 1123, RFC 
1141, RFC 1155, RFC 1157, RFC 1350, RFC 1533, RFC 1541, RFC 1542, RFC 1624, RFC 1700, RFC 
1867, RFC 2030, RFC 2616, RFC 2131, RFC 2132, RFC 3164, RFC 3411, RFC 3412, RFC 3413, RFC 
3414, RFC 3415, RFC 2576, RFC 4330, RFC 1213, RFC 1215, RFC 1286, RFC 1442, RFC 1451, RFC 
1493, RFC 1573, RFC 1643, RFC 1757, RFC 1907, RFC 2011, RFC 2012, RFC 2013, RFC 2233, RFC 
2618, RFC 2665, RFC 2666, RFC 2674, RFC 2737, RFC 2819, RFC 2863, RFC 1157, RFC 1493, RFC 
1215, RFC 3416

Proposed Device:
Make:							CISCO
Model:							SF300-24P
Price:							__________
Price configuration for myMix:				__________
Price Installation:					__________